



Basic screen.  


Limit case of 0.  


Limit case of 220.  


Shows that outside the range, target heart rate stops at 0.  


Normal input.  
